|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **# Test** | **Name** | **Description** | **Result** | **Succes** |
| 1 | Prevent text | Don't allow the user to input text for the distance and angle command | The interface ask to enter an interger whenever a command is added and letters figure in the input box. Thus, the input is discarded | Yes |
| 2 | Prevent other command | Don't allow the user to press any other command button (home, start,stop and send command) | The UI is disabled when one of those button is pressed. | Yes |
| 3 | Limit command number | A maximum of 6 command can be entered | When the user try to enter a 7th it discard it and tell the user that the list is full | Yes |
| 4 | Disable UI | Do not start any command when the UI is disabled | It works, but because our button are initialized with connect.clicked the UI remember that a button was clicked so the command start after the previous one finished | No |
| 5 | Servo angle | Limit the rotation of the servo because of physic limitation | When you enter an angle out off the -25 to 30 degree range an error indicate that the angle is out of reach | Yes |